**Pos.1 - SPECIFICATION FOR PROJECTOR**

|  | **Description** | **Requirement** | **Supplier’s Offer** |
| --- | --- | --- | --- |
| 1 | **Image** |  |  |
| 2 | Native Resolution | 1920 x 1080 |  |
| 3 | Maximum Resolution | 1920 x 1200 |  |
| 4 | Standard Mode Brightness | 3000 lm |  |
| 5 | Native Aspect Ratio | 16:09 |  |
| 6 | Compatible Aspect Ratio | 4:03 |  |
| 7 | Contrast Ratio | 10,000:1 |  |
| 8 | Throw Ratio | 0.5:1 (4.60 m@2000 mm) |  |
| 9 | Digital Zoom | 2x |  |
| 10 | Vertical Keystone Correction | -40°/+40° |  |
| 11 | Maximum Vertical Sync | 120 Hz |  |
| 12 | Maximum Horizontal Sync | 100 kHz |  |
| 13 | Minimum Vertical Sync | 24 Hz |  |
| 14 | Minimum Horizontal Sync | 15 kHz |  |
| 15 | Colour Supported | 1.07 Billion Colors (30-bit) |  |
| 16 | **Projection Lens** |  |  |
| 17 | Maximum Lens Aperture | F/2.8 |  |
| 18 | Maximum Focal Length | 7.42 mm |  |
| 19 | Minimum Diagonal Image Size | 1143 mm |  |
| 20 | Maximum Diagonal Image Size | 7.62 m (300") |  |
| 21 | Minimum Projection Distance | 500 mm |  |
| 22 | Maximum Projection Distance | 3.30 m |  |
| 23 | **Lamp** |  |  |
| 24 | Lamp Type | OSRAM |  |
| 25 | Number of Lamps | 1 |  |
| 26 | Lamp Power | 210 W |  |
| 27 | Normal Mode Lamp Life | 4000 Hour |  |
| 28 | Economy Mode Lamp Life | 6000 Hour |  |
| 29 | ExtremeEco Mode Lamp Life | 8000 Hour |  |
| 30 | **Interfaces/Ports** |  |  |
| 31 | HDMI | Yes |  |
| 32 | USB | Yes |  |
| 33 | Composite Video | Yes |  |
| 34 | VGA In | Yes |  |
| 35 | Audio Line In | Yes |  |
| 36 | Total Number of HDMI Ports | 2 |  |
| 37 | **Projection Method** | Ceiling, Front, Rear |  |
| 38 | **Video Compatibility** | EDTV, HDTV, NTSC, PAL, SDTV, SECAM |  |
| 39 | **Computer Compatibility** | Mac PC, Windows PC |  |
| 40 | 3D Capability | DLP 3D |  |
| 41 | **Audio** |  |  |
| 42 | Number of Speakers | 1 |  |
| 43 | Speaker Output Power | 2 W |  |
| 44 | Speaker Output Mode | Mono |  |
| 45 | **Power Description** |  |  |
| 46 | Power Supply | 100 V AC~240 V AC |  |
| 47 | Input Voltage | 230 V AC |  |
| 48 | Operating Power Consumption | 255 W |  |
| 49 | Operating Power Consumption (Eco Mode) | 196 W |  |
| 50 | Form Factor | Ceiling Mountable |  |
| 51 | **Miscellaneous** |  |  |
| 52 | Package Contents | H6517ST DLP Projector |  |
| 53 |  | AC Power Cord |  |
| 54 |  | Battery for Remote Control |  |
| 55 |  | Quick Start Guide |  |
| 56 |  | Remote Control |  |
| 57 |  | Security Card |  |
| 58 |  | User's Guide (CD-ROM) |  |
| 59 |  | VGA Cable |  |
| 60 | **Warranty** | Standard Warranty |  |

**Pos.6 - SPECIFICATION FOR TV 55 Inch**

|  | **Description** | **Requirement** | **Supplier’s Offer** |
| --- | --- | --- | --- |
| 1 | **Modeli** | SAMSUNG UE55RU7172UXXH |  |
| 2 | **Ekrani** |  |  |
| 3 | Diagonalja e ekranit: | 140 cm (55") |  |
| 4 | Tipi i HD: | 4K Ultra HD |  |
| 5 | Rezolucioni i ekranit: | 3840 x 2160 pixels |  |
| 6 | Teknologjija për interpolim: | PQI (Picture Quality Index) |  |
| 7 | Frekuenca e interpolimit (Hz): | 1400 Hz PQI |  |
| 8 | **Smart TV** |  |  |
| 9 | Smart TV: | PO |  |
| 10 | Sistemi operativ i instaluar: | Tizen |  |
| 11 | Versioni i sistemit operativ: | 5.0 |  |
| 12 | **Audio** |  |  |
| 13 | RMS fuqia e zërit (W): | 20 W |  |
| 14 | **Tjera** | \* 3 x HDMI; 2 x USB; Optical |  |
| 15 |  | \* Marrësi: DVB T2/C/S2 |  |
| 20 |  | \* UHD Dimming, HDR |  |
| 21 |  | \* Wi-Fi |  |
| 22 |  | \* UHD Processor |  |